WSDPrinterProbe

WSD printer enumeration probe

Sends out a WSD probe message for all printers configured to respond to WSD probe messages. Typically this is limited to 1 router hop, but this utility uses 2 hops as the default. You can modify the number of TTL hops on the command line, for example:

WSDPrinterProbe 3 Sets the TTL hops at 3

WSDPrinterProbe 2 Sets the TTL hops at 2

As the number of TTL router hops Is increased, you may find the printers returning back more variable. This is because the probe is UDP and network congestion along with the dropped packets would likely increase.