**AddIppPrinters**

Usage: AddIppPrinter /p=<printer IP address> /s=<631 or 443>

Adds an IPP/IPPS printer via IP address.

Usage: AddIppPrinter /l=<text file of ip addresses> /s=<631 or 443>

Opens the list and adds the IPP/IPPS printers based on IP addresses.

Note: The mandatory /s switch specifies IPP (port 631) or IPPS (port 443)

If 631 is chosen and the printer supports IPPS, STARTTLS will be employed to ensure TLS is used.

Example: **/l=C:\Temp\Printers.txt /s=443**

Adds all the printers listed in Pinters.txt as IPPS printers using port 443.

Example: **/l=C:\Temp\Printers.txt /s=631**

Adds all the printers listed in Pinters.txt as IPP printers on port 631..